Step before Autotuning:

1. Temperature setpoint should be operating temperature and at least 10 degree above room temperature
2. heater should be turned on and up to setpoint and stable
3. slope change should be low and wait for 5 mins
4. autotune start, the output should be more than 20%